SECTION 09 29 00 – GYPSUM BOARD, 1/4 in. (6.4 mm) and 3/8 in. (9.5 mm) USG Sheetrock® Brand Gypsum Panels

|  |
| --- |
| **Product Summary:** |
| * 1/4 in. (6.4 mm) panels are recommended as an additional layer for improving sound control in double-layer wood- or steel-framed partitions, and as a face layer for use over old wall and ceiling surfaces
* 3/8 in. (9.5 mm) panels are recommended in single- or double-layer wood- or steel-framed wall and ceilings, as an additional layer for improving sound control, and as a face layer for use over old wall and ceiling surfaces
* Feature a noncombustible gypsum core that is encased in 100% recycled face and back papers that form a high strength composite design
* Comply with ASTM C1396, *Standard Specification for Gypsum Board*, for 1/4 in. (6.4 mm) and 3/8 in. (9.5 mm) gypsum wallboard
* Underwriters Laboratories Inc. (UL) Classification as to surface-burning characteristics and noncombustibility
* Achieved GREENGUARD Gold Certification and qualifies as a low VOC emitting material (meets CA 01350)
* For more information, refer to product submittal sheet WB1473 and usg.com
 |

|  |
| --- |
| **Note to Specification Writers:**  |
| * This document is not intended to function as a standalone specification. It is intended to assist the specifier in inserting the proper language into the following recommended specification sections: 09 29 00 – GYPSUM BOARD.
* This product is manufactured at USG gypsum panel plants, reducing distances and carbon footprint for transport.
* Panels shall be installed in accordance with GA-216, *Specifications for the Application and Finishing of Gypsum Panel Products* and ASTM C840, *Standard Specification for Application and Finishing of Gypsum Board*.
* Contact USG at800.874.4968 for technical questions.
 |

PART 2 – GYPSUM PANEL PRODUCTS

* + - 1. GYPSUM PANEL
				1. ASTM C1396, *Standard Specification for Gypsum Board*, for 1/4 in. (6.4 mm) and 3/8 in. (9.5 mm) gypsum wallboard

Basis of Design: Subject to compliance with project requirements, the design is based on the following: United States Gypsum Company, USG Sheetrock® Brand Gypsum Panels

UL Type Designation: [1/4 in. (6.4 mm): Not applicable] [3/8 in. (9.5 mm): Not applicable]

ASTM E136 Noncombustibility: Meets

ASTM E84 Surface-Burning Characteristics

Flame Spread: [1/4 in. (6.4 mm): 15] [3/8 in. (9.5 mm): 15]

Smoke Developed: [1/4 in. (6.4 mm): 0] [3/8 in. (9.5 mm): 0]

Class A (Flame spread not greater than 25 and smoke developed not greater than 450): Meets

ASTM C473, *Standard Test Methods for Physical Testing of Gypsum Panel Products*

Core Hardness

Field: {1/4 in. [6.4 mm] (Not less than 11 lbf (49 N)): Meets} {3/8 in. [9.5 mm] (Not less than 11 lbf (49 N)): Meets}

End: {1/4 in. [6.4 mm] (Not less than 11 lbf (49 N)): Meets} {3/8 in. [9.5 mm] (Not less than 11 lbf (49 N)): Meets}

Edge: {1/4 in. [6.4 mm] (Not less than 11 lbf (49 N)): Meets} {3/8 in. [9.5 mm] (Not less than 11 lbf (49 N)): Meets]

Flexural Strength

Parallel: {1/4 in. [6.4 mm] (Not less than 16 lbf (71 N)): Meets} {3/8 in. [9.5 mm] (Not less than 26 lbf (116 N)): Meets}

Perpendicular: {1/4 in. [6.4 mm] (Not less than 46 lbf (205 N)): Meets} {3/8 in. [9.5 mm] (Not less than 77 lbf (343 N)): Meets}

Nail Pull Resistance: {1/4 in. [6.4 mm] (Not less than 36 lbf (160 N)): Meets} {3/8 in. [9.5 mm] (Not less than 56 lbf (249 N)): Meets}

Humidified Deflection: {1/4 in. [6.4 mm] (Not required): Meets} {3/8 in. [9.5 mm] (Not greater than 1-7/8 in. (48 mm)): Meets}

Thickness: [1/4 in. (6.4 mm)] [3/8 in. (9.5 mm)]

Length: 8-16 ft. (2438-4877 mm)

Width: 4 ft. (1219 mm)

Weight: [1/4 in. (6.4 mm): 1.2 lb./sq. ft. (5.9 kg/sq. m.)] [3/8 in. (9.5 mm): 1.4 lb./sq. ft. (6.8 kg/sq. m.)]

Edge: Tapered

Disclaimer: The USG Product Specifications contained herein are intended for use as product reference material by architects, engineers, other design professionals, contractors, building code officials, or other competent construction industry trade professionals having an interest in the selection, specification and use of products manufactured by the subsidiaries of USG Corporation. The specifications are intended solely as technical support incident to the sale and use of USG products and not intended to be a substitute for the design review and approval of the licensed design professionals for the project. These materials may be printed and/or transferred electronically solely as needed by the user. Because electronic files can be modified by other parties, without notice or indication of such modifications, modification of USG Product Guide Specifications is the sole responsibility of the Design Professional.