SECTION 09 51 00 – USG COMPÄSSO™ ELITE FOR DRYWALL ALUMINUM PERIMITER TRIM

|  |
| --- |
| **Product Summary:** |
| * USG Compässo™ Elite for Drywall is an extruded aluminum trim for creating drywall ceiling fascias. * Easier to install than conventional drywall fascias. * Available in 2-1/2", 4", 6" and 8" trim heights. * Integrated taping flange for a clean, finished edge. * Designed for 5/8" thick gypsum board. * Works with USG Compässo™ Elite attachment clips and splice plates * Call **<insert product representative here>** or 800.874.4968 for technical questions. |

|  |
| --- |
| **Note to Specifier:** |
| * This document is not intended to function as a standalone specification. It is intended to assist the specifier in inserting the proper language into the following recommended specification sections:   + 09 51 13 Acoustical Panel Ceilings, Accessories.   + 09 51 23 Acoustical Tile Ceilings, Accessories.   + 09 51 33 Acoustical Metal Pan Ceilings, Accessories.   + 09 54 23 Linear Metal Ceilings, Accessories. |

Note to Specifier: This language is to be inserted into section 2.6 ACCESSORIES: METAL EDGE MOLDING AND TRIM.

2.6 COMPÄSSO™ ELITE METAL EDGE TRIM FOR DRYWALL <Insert material designation>.

Note: Provide USG Compässo™ Elite for Drywall extruded aluminum edge moldings and trim: where indicated. The aluminum trim will feature smooth visible face with reveal edges on the upper return side. The lower return side shall feature an integrated drywall bead edge. The non-visible face shall include extruded bosses to accommodate Compässo™ Elite attachment clips that attach trim to adjacent ceiling grid. At vertical butt joints between adjacent trim pieces, utilize Compässo™ splice clips. Prefabricated corner pieces accommodate inwards and outwards 90 degree corners.

* + - * 1. Basis of Design: Subject to compliance with project requirements, the design is based on the following: USG Interiors, LLC, **“USG COMPÄSSO™ ELITE FOR DRYWALL ALUMINUM TRIM”.**

Trim Height: [2-1/2” (62 mm)] [4” (102 mm)] [6” (152 mm)] [8” (203 mm)].

Trim Depth: 1” (25 mm).

Trim Length: 10’-0” (3048 mm).

Color: Primer white.

* + - * 1. Accessories:

Compässo™ Elite Attachment Clip; attaches grid to backside bosses on Compässo™ Elite Trim. Note: at vertical butt joints, provide (1) at 2”, (2) with 4” and 6” and (3) with 8” and 10” trims.

Splice Plate: steel in finish to match trim pans; formed for snap-fit into 8" pan ends, for use at cut ends of metal ceilings.

90° corner trim pieces: to match Compässo™™ Elite Suspension Trim.

USG Ceilings Compässo™ Elite for Drywall, 90 degree Inside Corner, Flat **<insert color here>**.

USG Ceilings Compässo™ Elite for Drywall, 90 degree Outside Corner, Flat **<insert color here>**.

END OF SECTION

Disclaimer: The USG Product Specifications contained herein are intended for use as product reference material by architects, engineers, other design professionals, contractors, building code officials, or other competent construction industry trade professionals having an interest in the selection, specification and use of products manufactured by the subsidiaries of USG Corporation. The Specifications are intended solely as technical support incident to the sale and use of USG products and not intended to be a substitute for the design review and approval of the licensed design professionals for the project. These materials may be printed and/or transferred electronically solely as needed by the user. Because electronic text files can be modified by other parties, without notice or indication of such modifications, modification of USG Product Guide Specifications and Drawings is the sole responsibility of the Design Professional.