1. Section 095100
DIRECT-APPLIED ACOUSTICAL PERFORATED GYPSUM CEILING PANELS - USG
	1. PART 1  GENERAL
		1. SECTION INCLUDES
			1. Suspended metal grid ceiling systems.
			2. Acoustical and nonacoustical units.
2. *The paragraph below is optional text*
	* + 1. Supplementary acoustical insulation above ceiling.
			2. Wall angles and shadow moldings.
3. *The paragraph below is optional text*
	* + 1. Special trims and accessories.
		1. RELATED REQUIREMENTS
4. *The paragraph below is optional text*
	* + 1. Section 016116 - Volatile Organic Compound (VOC) Content Restrictions.
5. *The paragraph below is optional text*
	* + 1. Section 031000 - Concrete Forming and Accessories:  Placement of special anchors or inserts for suspension system.
6. *The paragraph below is optional text*
	* + 1. Section 033000 - Cast-in-Place Concrete:  Placement of special anchors or inserts for suspension system.
7. *The paragraph below is optional text*
	* + 1. Section 053100 - Steel Decking:  Placement of special anchors or inserts for suspension system.
			2. Section 072100 - Thermal Insulation.
			3. Section 092116 - Gypsum Board Assemblies:  Acoustical insulation.
			4. Section 095153 - Direct-Applied Acoustical Ceilings.
			5. Section 211300 - Fire-Suppression Sprinkler Systems:  Sprinkler heads.
			6. Section 233700 - Air Outlets and Inlets:  Air diffusion devices.
			7. Section 265100 - Interior Lighting:  Light fixtures.
			8. Section 275116 - Public Address Systems:  Speakers.
			9. Section 284600 - Fire Detection and Alarm:  Fire alarm components.
		1. REFERENCE STANDARDS
			1. ASTM A580/A580M - Standard Specification for Stainless Steel Wire; 2018.
			2. ASTM A653/A653M - Standard Specification for Steel Sheet, Zinc-Coated (Galvanized) or Zinc-Iron Alloy-Coated (Galvannealed) by the Hot-Dip Process; 2022.
			3. ASTM B209/B209M - Standard Specification for Aluminum and Aluminum-Alloy Sheet and Plate; 2021a.
			4. ASTM C423 - Standard Test Method for Sound Absorption and Sound Absorption Coefficients by the Reverberation Room Method; 2022.
			5. ASTM C635/C635M - Standard Specification for Manufacture, Performance, and Testing of Metal Suspension Systems for Acoustical Tile and Lay-in Panel Ceilings; 2022.
			6. ASTM C636/C636M - Standard Practice for Installation of Metal Ceiling Suspension Systems for Acoustical Tile and Lay-In Panels; 2019.
			7. ASTM E84 - Standard Test Method for Surface Burning Characteristics of Building Materials; 2023.
			8. ASTM E119 - Standard Test Methods for Fire Tests of Building Construction and Materials; 2022.
8. *The paragraph below is optional text*
	* + 1. ASTM E413 - Classification for Rating Sound Insulation; 2022.
			2. ASTM E1264 - Standard Classification for Acoustical Ceiling Products; 2022.
			3. UL (GGG) - GREENGUARD Gold Certified Products; Current Edition.
		1. ADMINISTRATIVE REQUIREMENTS
			1. Coordination:  Coordinate work of this section with installation of mechanical and electrical components and with other construction activities affected by work of this section.
				1. Review with affected installers those locations of facility services lines and equipment within ceiling plenum that prevent installation of hangers at spacings compliant with limitations established in referenced standards.  Arrange for each affected mechanical or electrical installer to provide necessary number of additional structural support points for ceiling installer.
			2. Preinstallation Meeting:  Convene one week before starting work of this section.
			3. Sequencing:  Schedule work of affected trades to minimize or eliminate installation conflicts and rework.
				1. Supply hanger clips during steel deck erection.  Supply additional hangers and inserts as required.
				2. Ensure that acoustical ceilings are not installed until building is enclosed, sufficient heat is provided, dust generating activities have terminated, and overhead work is completed, tested, and approved.  Do not install acoustical units until after interior wet work is dry.
		2. SUBMITTALS
			1. See Section 013000 - Administrative Requirements for submittal procedures.
			2. Shop Drawings:  Indicate grid layout and related dimensioning.
			3. Product Data:  Provide data on suspension system components and acoustical units.
			4. Samples:  Two samples [\_\_\_\_\_] by [\_\_\_\_\_] inches ([\_\_\_\_\_] by [\_\_\_\_\_] mm) in size indicating material and finish of acoustical units.
			5. Samples:  Two samples each, [\_\_\_\_] inches ([\_\_\_\_] mm) long of suspension system main runner, cross runner, and perimeter molding.
9. *The paragraph below is optional text*
	* + 1. Manufacturer's Installation Instructions:  Indicate special procedures and perimeter conditions requiring special attention.
			2. Designer's qualification statement.
			3. Installer's qualification statement.
			4. Maintenance Materials:  Furnish the following for Owner's use in maintenance of project.
10. *The paragraph below is optional text*
	* + - 1. See Section 016000 - Product Requirements for additional provisions.
11. *The paragraph below is optional text*
	* + - 1. Extra Acoustical Units:  [\_\_\_\_] sq ft ([\_\_\_\_] sq m) of each type and size.
12. *The paragraph below is optional text*
	* + - 1. Extra Acoustical Units:  Quantity equal to 5 percent of total installed.
		1. QUALITY ASSURANCE
			1. Designer Qualifications for Seismic Design:  Perform under direct supervision of a Professional Structural Engineer experienced in design of this work and licensed in the State in which the Project is located.
			2. Installer Qualifications:  Company specializing in performing work of the type specified and with at least three years of documented experience and approved by manufacturer.
		2. FIELD CONDITIONS
			1. Maintain uniform temperature of minimum 60 degrees F (16 degrees C), and maximum humidity of 40 percent before, during, and after acoustical unit installation.
	1. PART 2  PRODUCTS
		1. CEILING ASSEMBLIES
			1. Acoustical Ceiling Assembly Type APC-1:
				1. Acoustical Units:  Danoline Perforated Gypsum 1/2" Direct-Mount, Item No. [22749],[22750],[22752].

Panel Size: [[36] inches by [96] inches ([914.4] mm by [2438.4] mm)] [[48] inches by [96] inches ([1219.2] mm by [2438.4] mm)].

Panel Edge:  SQ edge.

Color:  Flat White RAL 9003.

Perforations:

Patterns and Geometry: [3L1 (3 Feet x 8 Feet) 01 Obround 5/32 Inch x 9/16 Inch (4X14mm)] [2L2 (4 Feet x 8 Feet) S9 Square 3/8 Inch (9mm)] [2L2 (4 Feet x 8 Feet) S12 Square 1/2 Inch (12mm)]

Open Areas: [15.5% (01 Panel)] [15% (S9 Panel)] [12.2% (S12 Panel)

Characteristics:  Noise Reduction Coefficient = [N/A], Ceiling Attenuation Class = [N/A], Light Reflectance = [69.2] [72.8], Recycled Content = [N/A], Environmental Product Declaration: [N/A], Health Product Declaration: [N/A], GreenGuard Gold: [Yes], EC3 Score: [N/A], ClimaPlus Warranty: [N/A].

* + - * 1. Danoline Acoustical Drywall Ceiling

Color:  White.

Support Assembly:  Direct-mount system.

* + 1. Ceiling PERFORMANCE REQUIREMENTS
			1. Design for maximum deflection of 1/360 of span.
			2. Fire-Resistance Rating:  Determined in accordance with test procedures in ASTM E119 and complying with the following:
1. *The paragraph below is optional text*
	* + - 1. UL (FRD) Assembly Design No. [\_\_\_\_].
2. *The paragraph below is optional text*
	* + - 1. ICC-ES Evaluation Report No. [\_\_\_\_\_\_\_\_\_\_].
			1. Seismic Performance:  Ceiling systems designed to withstand the effects of earthquake motions determined according to ASCE 7 for Seismic Design Category D, E, or F and complying with the following:
3. *The paragraph below is optional text*
	* + - 1. Local authorities having jurisdiction.
4. *The paragraph below is optional text*
	* + - 1. ICC-ES Evaluation Report No. [\_\_\_\_\_\_\_\_\_\_].
		1. Ceiling COMPONENT PRODUCTS
			1. Acoustical Units:
				1. Acoustical Units - General:  ASTM E1264, Fire Class A.

VOC Content:  As specified in Section 016116.

VOC Content:  Certified as Low Emission by one of the following:

Product listing in UL (GGG).

Product listing in CHPS (HPPD).

Noise Reduction Coefficient (NRC) rating, Ceiling Attenuation Class (CAC) rating, and Light Reflectance Coefficient (LR) performance for each type of unit specified below, as determined in accordance with ASTM E1264.

Fire Class / Surface Burning Characteristics:  Determined in accordance with test method ASTM E84.

Surface Burning Characteristics:  Unless otherwise indicated, flame spread index of 25 or less, smoke developed index of 50 or less.

* + - * 1. Acoustical Panels:  Precision-perforated gypsum boards, with the following characteristics:

Classification:  ASTM E1264 Type XX.

Pattern(s):  Includes the following, as applicable to each product specified.

A - Perforated, regularly spaced large holes.

Thickness:  1/2 inch (13 mm).

Recycled Content:  As applicable to selected products.

Material Ingredients Transparency:  Products included in the USG EcoBlueprint Program.

Low Emissions (VOC):  Greenguard-certified products.

Panel Edge:  [SQ].

Perforation Pattern:  [O1],[S12],[S9].

Perforation Layout:  [2L2],[3L1].

Products:

USG Corporation; Danoline Acoustical Perforated Gypsum Direct-Mount Panels:  www.usg.com/ceilings/#sle.

Substitutions:  Not permitted.

* + - 1. Suspension Systems:
				1. Metal Suspension Systems - DWSS Drywall Suspension System:  Complying with ASTM C635/C635M; die cut and interlocking components, with [splices], [attachment clips], [wall angles and moldings] as required.
				2. Enclosure for Recessed Ceiling Fixtures:  Mineral fiber insulation box enclosure with foil facing on exterior side for placement over recessed ceiling light fixture; flame spread index of 25 and smoke development index of 0 (zero) when tested in accordance with ASTM E84.

Manufacturers:

[\_\_\_\_\_\_].

Substitutions:  See Section 016000 - Product Requirements.

* + - 1. Direct Mount System:  Attachment directly to structural deck using CMAC-1 Close Mount Attachment Clips and appropriate fasteners.
1. *The paragraph below is optional text*

Color:  As indicated on drawings.

1. *The paragraph below is optional text*
	* + 1. Moldings and Trim:
2. *The paragraph below is optional text*
	* + - 1. Edge Molding, Expansion Joints, and Splices - General:  Same material, thickness, and finish as metal pan panels, unless otherwise indicated.
				2. Perimeter Wall Moldings:  Same metal and finish as grid.
3. *The paragraph below is optional text*

Size:  As required for installation conditions.

1. *The paragraph below is optional text*

Angle Moldings:  L-shaped, for mounting at same elevation as face of grid.

1. *The paragraph below is optional text*

Shadow Moldings:  Shaped to create a perimeter reveal.

1. *The paragraph below is optional text*

Channel Moldings:  U-shaped, for hold-down type installations.

1. *The paragraph below is optional text*

Gaskets For Perimeter Moldings:  Closed-cell foam, factory-applied to molding.

1. *The paragraph below is optional text*

Acoustical Sealant For Perimeter Moldings:  Nonhardening, nonskinning, for use in conjunction with suspended ceiling system.

1. *The paragraph below is optional text*
	* + - 1. Metal Transition Trim:  Steel or extruded aluminum; provide attachment clips, splice plates and preformed corner pieces for complete trim system.
2. *The paragraph below is optional text*

Trim Height:  6 inch (152 mm).

1. *The paragraph below is optional text*

Finish:  Baked enamel.

1. *The paragraph below is optional text*

Color:  White.

1. *The paragraph below is optional text*

Accessories: [CMAC-1 Close Mount Attachment Clip], [Splice Clip], [Transition Clip], [Wall Attachment Clip], [USG Compasso Drywall Clip].

1. *The paragraph below is optional text*

Products:

1. *The paragraph below is optional text*

USG Corporation; DWSS Drywall Suspension System – Flat Ceilings:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

USG Corporation; DWSS Drywall Suspension System - Acoustical to Drywall:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

USG Corporation; DWSS Drywall Suspension System – Direct Mount:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

[\_\_\_\_\_\_].

1. *The paragraph below is optional text*

Substitutions:  Not permitted.

1. *The paragraph below is optional text*
	* + - 1. Metal Perimeter Trim for "Cloud" Suspension Systems:  Steel or extruded aluminum; provide attachment clips, splice plates, and preformed corner pieces for complete trim system.
2. *The paragraph below is optional text*

Trim Height:  [2-1/4 inches (58 mm)], [4 inches (102 mm)], [6 inches (152 mm)], [8 inches (203 mm)], [10 inches (254 mm)], [12 inches (305 mm)].

1. *The paragraph below is optional text*

Finish:  Baked enamel.

1. *The paragraph below is optional text*

Color:  White.

1. *The paragraph below is optional text*

Products:

1. *The paragraph below is optional text*

USG Corporation; Compasso Suspension Trim - Standard:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

USG Corporation; Compasso Suspension Trim - Slim:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

USG Corporation; Compasso Suspension Trim - Elite:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

USG Corporation; Compasso Suspension Trim - Elite with Island Accent Lighting:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

[\_\_\_\_\_\_].

1. *The paragraph below is optional text*

Substitutions:  Not permitted.

* + - * 1. Metal Curtain Pocket Trim:  Steel or extruded aluminum; provide attachment clips, splice plates, and preformed corner pieces for complete trim system.
1. *The paragraph below is optional text*

Type:  Three-sided.

1. *The paragraph below is optional text*

Closure Plate Size:  2 inches (51 mm).

1. *The paragraph below is optional text*

Extension Trim Height:  6 inches (152 mm).

1. *The paragraph below is optional text*

Finish:  Baked enamel.

1. *The paragraph below is optional text*

Color:  White.

Products:

1. *The paragraph below is optional text*

USG Corporation; Compasso Elite Curtain Pocket:  www.usg.com/ceilings/#sle.

1. *The paragraph below is optional text*

Substitutions:  Not permitted.

* + 1. ACOUSTICAL WALL SYSTEMS
			1. Acoustical and thermal insulation made from inorganic glass fibers preformed into boards with ECOSE technology.
				1. Installation Accessories:  Manufacturer's standard.
1. *The paragraph below is optional text*
	* + - 1. Products:
2. *The paragraph below is optional text*

Knauf Insulation; Acoustical Smooth Board with ECOSE Technology:  www.knaufnorthamerica.com/ceilings/#sle.

Knauf Insulation; Black Acoustical Board with ECOSE Technology:  www.knaufnorthamerica.com/ceilings/#sle.

[\_\_\_\_\_\_\_\_\_\_].

Substitutions:  Not permitted.

1. *The paragraph below is optional text*
	* 1. ACCESSORIES
2. *The paragraph below is optional text*
	* + 1. Support Channels, Carriers, and Hangers:  Galvanized steel; size and type to suit application and ceiling system flatness requirement specified.
3. *The paragraph below is optional text*
	* + 1. Hat-Shaped Metal Channels:  Steel, 22 gauge, 0.0299 inch (0.76 mm), minimum.
4. *The paragraph below is optional text*
	* + 1. Suspension Wire:  Size and type as required for application, seismic requirements, and ceiling system flatness requirement specified.
5. *The paragraph below is optional text*
	* + - 1. Concealed Suspension:

Suspension Wire:  Steel, annealed, galvanized finish, 12 gauge, 0.0808 (2.05 mm) diameter, complying with ASTM A641/A641M.

1. *The paragraph below is optional text*
	* + - 1. Exposed (To View) Suspension:
2. *The paragraph below is optional text*

Suspension Wire:  Stainless steel, 18 gauge, 0.0403 (1.02 mm) diameter, complying with ASTM A580/A580M.

1. *The paragraph below is optional text*

Suspension Rope:  1/32 inch (0.8 mm) stainless steel rope wire complying with ASTM A492, with [loop and crimp-end],[turnbuckle] connection.

1. *The paragraph below is optional text*
	* + 1. Compression Framing and Bracing:  Metal stud sizes, gauges, and spacings as determined by qualified structural design professional and complying with applicable codes.
2. *The paragraph below is optional text*
	* + 1. Compression Posts: 3.4 inch (19 mm) nominal diameter EMT conduit, lengths as required by installation conditions.
3. *The paragraph below is optional text*
	* + - 1. Adapters:  Manufacturer's standard adapters designed to connect post to suspension carrier member.
4. *The paragraph below is optional text*
	* + 1. Hold-Down Clips:  Manufacturer's standard clips to suit application.
5. *The paragraph below is optional text*
	* + 1. Seismic Clips:  Manufacturer's standard clips for seismic conditions and to suit application.
6. *The paragraph below is optional text*
	* + 1. Drywall Ceiling Installation Accessories:  Products recommended by gypsum board manufacturer.
7. *The paragraph below is optional text*
	* + - 1. Close Mount Attachment Clips:  Manufacturer's standard clips used in tight plenum applications to provide strong deck support connection without the use of hanger wires.
8. *The paragraph below is optional text*
	* + 1. Unopposed Tee Attachment Clip:  Manufacturer's standard clip designed to create code-compliant cross tee connections when a cross tee is installed in a main tee without another cross tee directly opposite ("ashlar" installations).
9. *The paragraph below is optional text*
	* + 1. Compasso Standard clip.
10. *The paragraph below is optional text*
	* + 1. Compasso Celebration clip.
11. *The paragraph below is optional text*
	* + 1. Compasso Elite clip.
12. *The paragraph below is optional text*
	* + 1. Celebration Compasso Elite clip.
13. *The paragraph below is optional text*
	* + 1. Glass Fiber Boards:  Smooth, preformed boards made from inorganic glass fibers, complying with ASTM C665.
14. *The paragraph below is optional text*
	* + - 1. Smoke Developed Index:  50 or less, when tested in accordance with ASTM E84.
15. *The paragraph below is optional text*
	* + - 1. Sustainability Certifications:  Greenguard Gold Certified; Declare Red List Free.
				2. Formaldehyde Content:  Zero, as validated by UL.
16. *The paragraph below is optional text*
	* + - 1. Thickness:  As indicated on drawings.
17. *The paragraph below is optional text*
	* + - 1. Thickness: [3/4 inches (19 mm)], [1 inch (25 mm)], [1-1/2 inches (38 mm)], [2 inches (51 mm)]..
				2. Products:
18. *The paragraph below is optional text*

Knauf Insulation Inc; Knauf Smooth Board with ECOSE Technology:  www.knaufnorthamerica.com/#sle.

1. *The paragraph below is optional text*

[\_\_\_\_\_\_].

1. *The paragraph below is optional text*

[\_\_\_\_\_\_].

1. *The paragraph below is optional text*

Substitutions:  Not permitted.

1. *The paragraph below is optional text*
	* + 1. Thermal Insulation:  Specified in Section 072100.
			2. Thermal Insulation:  ASTM C665,  preformed glass fiber batt; friction fit, complying with the following:
2. *The paragraph below is optional text*
	* + - 1. Thermal Resistance:  R-value (RSI-value) of [\_\_\_\_] ([\_\_\_\_]).
3. *The paragraph below is optional text*
	* + - 1. Batt Size:  [\_\_\_]  by [\_\_\_] inch ([\_\_\_]  by [\_\_\_] mm).
4. *The paragraph below is optional text*
	* + - 1. Facing:  Unfaced at [\_\_\_\_\_].
5. *The paragraph below is optional text*
	* + - 1. Facing:  Faced on one side with foil at [\_\_\_\_\_].
6. *The paragraph below is optional text*
	* + 1. Gypsum Board and Framing Materials:  See Section 092116.
			2. Touch-Up Paint for Exposed Surfaces:  Type and color to match acoustical units and suspension system grid and trim elements.
			3. Touch-Up Paint For Concealed Items:  Zinc rich type, as recommended by ceiling system manufacturer.
		1. Fabrication
			1. Shop fabricate ceiling components to the greatest extent possible.
			2. Fabricate components to allow access to ceiling plenum as required.
	1. PART 3  EXECUTION
		1. EXAMINATION
			1. Verify existing conditions before starting work.
			2. Verify that layout of hangers will not interfere with other work.
			3. Verify that field measurements are as indicated on shop drawings.
			4. Start of installation constitutes acceptance of project conditions.
		2. Preparation
			1. Coordinate the location of hangers with other work.
			2. Provide hanger clips during steel deck erection.  Provide for anticipated additional hangers and inserts as required.
7. *The paragraph below is optional text*
	* + 1. Install ceiling system after major above-ceiling work is complete.
			2. Acclimate wood ceiling materials by removing from packaging in installation area a minimum of 72 hours prior to installation.
		1. INSTALLATION - SUSPENSION SYSTEM
8. *The paragraph below is optional text*
	* + 1. Install suspension system in accordance with ASTM C636/C636M and manufacturer's instructions and as supplemented in this section.
9. *The paragraph below is optional text*
	* + 1. Install hangers and inserts coordinated with overhead work.  Provide additional hangers and supports as required.
			2. Rigidly secure system, including integral mechanical and electrical components, for maximum deflection of 1:360.
			3. Lay out system to a balanced grid design with edge units no less than 50 percent of acoustical unit size.
10. *The paragraph below is optional text*
	* + 1. Locate system on room axis according to reflected ceiling plan.
			2. Suspension System, Nonseismic:  Hang suspension system independent of walls, columns, ducts, pipes and conduit.  Where carrying members are spliced, avoid visible displacement of face plane of adjacent members.
			3. Seismic Suspension System, Seismic Design Category C:  Hang suspension system independent of walls, columns, ducts, pipes and conduit.  Maintain a 3/8 inch (9 mm) clearance between grid ends and wall.
			4. Seismic Suspension System, Seismic Design Categories D, E, F:  Hang suspension system with grid ends attached to the perimeter molding on two adjacent walls; on opposite walls, maintain a 3/4 inch (19 mm) clearance between grid ends and wall.
			5. Where ducts, facility services, or equipment prevent the regular spacing of hangers, reinforce the nearest affected hangers and related carrying channels to span the extra distance.
			6. Do not support components on main runners or cross runners if weight causes total dead load to exceed deflection capability.
			7. Support fixture loads using supplementary hangers located within 6 inches (152 mm) of each corner, or support components independently.
			8. Do not eccentrically load system or induce rotation of runners.
11. *The paragraph below is optional text*
	* + 1. Form expansion joints as detailed.  Form to accommodate plus or minus 1 inch (25 mm) movement.  Maintain visual closure.
			2. Edge Moldings:  Install at intersection of ceiling and vertical surfaces and penetrations, using components of maximum length; set level. Provide edge moldings at junction with other ceiling finishes. Miter corners. Provide preformed edge closures to match bullnosed cornered partitions.
				1. Install in bed of acoustical sealant.
				2. Use longest practical lengths.
				3. Overlap and rivet corners.
			3. Install light fixture boxes constructed of gypsum board above light fixtures in accordance with fire rated assembly requirements and light fixture ventilation requirements.
		1. INSTALLATION - ACOUSTICAL UNITS
			1. Install acoustical units in accordance with manufacturer's instructions.
			2. Fit acoustical units in place, free from damaged edges or other defects detrimental to appearance and function.
			3. Fit edge trim neatly against abutting surfaces.
			4. Install acoustical units level, in uniform plane, and free from twist, warp, and dents.
			5. Cutting Acoustical Units:
				1. Cut to fit irregular grid and perimeter edge trim.
				2. Make field cut edges of same profile as factory edges.
			6. Lay acoustical insulation for a distance of 48 inches (1219 mm) either side of acoustical partitions as indicated.
			7. Install hold-down clips on acoustical units within 20 ft (6 m) of an exterior door.
		2. INSTALLATION OF TRANSITION TRIM
12. *The paragraph below is optional text*
	* + 1. After the grids are installed, for each grid end that meets the transition trim, insert one tee attachment clip into the lower and upper bosses and secure the set screw. Leave enough tension for adjustment.
13. *The paragraph below is optional text*
	* + 1. At drywall suspension systems install gypsum panels after the transition trim is installed.
14. *The paragraph below is optional text*
	* + 1. Secure a tee attachment clip to each grid member that will connect to the transition trim. Install one framing screw into the center of the slotted screw hole. Leave enough tension so the attachment clip can be adjusted if needed. Follow manufacturer's instructions when aligning the attachment clip.
15. *The paragraph below is optional text*
	* + 1. Install the splice plates by sliding them into the bosses at the end of each transition trim joint. Loosely tighten the set screws and align the system square and true.
16. *The paragraph below is optional text*
	* 1. INSTALLATION OF Perimeter "Cloud" TRIM
17. *The paragraph below is optional text*
	* + 1. General:  Install in accordance with manufacturer's instructions.
18. *The paragraph below is optional text*
	* + - 1. Examine the reflected ceiling layout and carefully plan the layout of the trim on the ceiling grid.
				2. Lay trim segments on top of the grid in the desired pattern and temporarily secure them in place.
19. *The paragraph below is optional text*
	* + - 1. Temporarily splice the segments together.
20. *The paragraph below is optional text*
	* + - 1. Assemble trim system, arranging the trim into smooth curves.
				2. Mark and cut the suspension grid.
21. *The paragraph below is optional text*
	* + - 1. Install an attachment clip to each cut end of the grid. Attach the clip to trim section segment.
22. *The paragraph below is optional text*
	* + - 1. Join trim and permanently splice the segments together.
			1. 10-Inch and 12-Inch Trim:
				1. Support segments by attaching diagonal braces to the installation clips using fasteners recommended by manufacturer.  Attach one end of the brace to back of trim segment and the other to the tee. Ensure that the clip remains at 90 degrees to the ceiling plane. Repeat this procedure at  24 inches (610 mm) increments along the entire perimeter of the grid.
				2. Attach trim segments to the grid.
23. *The paragraph below is optional text*
	* + 1. Corners:
24. *The paragraph below is optional text*
	* + - 1. Outside Corners:  Slide a permanent splice plate into each side of the preformed outside corner. Attach one side of the outside corner to a trim segment. Connect a trim segment to the other side of the corner and secure with appropriate splice plate.
				2. Inside Corners:  Follow manufacturer's instructions for installation of preformed and welded corners or for field-assembled corners from separate premitered pieces.
25. *The paragraph below is optional text*
	* 1. TOLERANCES
			1. Maximum Variation from Flat and Level Surface:  1/8 inch in 10 feet (3 mm in 3 m).
			2. Maximum Variation from Plumb of Grid Members Caused by Eccentric Loads:  Two degrees.
		2. Cleaning
			1. Clean and touch up minor finish damage.  Remove and replace components that cannot be successfully cleaned and repaired.
26. END OF SECTION