SECTION 095123 – USG SANDRIFT™ BASIC ACOUSTICAL TILE CEILINGS

USG SANDRIFT™ BASIC

* Uniquely textured cast product with durable surface that resists scrapes commonly caused by accessing the ceiling plenum. Integral color masks nicks and scratches.
* Zero VOC emissions exceeds CA Specification 01350.
* Optional Firecode® product designed to meet life safety codes
* USDA Certified Biobased Product
* **<insert product representative here>** or 800.874.4968 for technical questions

**Note to specifiers:**

This document is not intended to function as a standalone specification. It is intended to assist the specifier in inserting the proper language into the following recommended specification sections:

* 09 51 13 Acoustical Panel Ceilings
* 09 51 23 Acoustical Tile Ceilings

2.3 ACOUSTICAL TILES

* + - * 1. Acoustical Panel Type **<INSERT DESIGNATION HERE>**:

Basis of Design: Subject to compliance with project requirements, the design is based on the following: USG Interiors, LLC, “Sandrift Basic”.

Classification: Provide ceiling panels complying with ASTM E 1264 for type, form and pattern as follows:

Type: III, mineral base with painted finish

Form: 4, Cast or Molded

Pattern: Z, Patterned

Color: **[Flat White 050] [Beige 142] [Charcoal 534] [Flat Black 205] [Manila 246] [Mist 053] [Parchment 103] [Sandstone 090] [Silvertone 052] [Straw 143] [Taupe 107] [Azure 2660] [Blue Grey 564] [Breeze 2859] [Halo 206] [Nectar 546] [Quartz 082] [Redwood 566] [Sienna 565] [Safari 2662] [Slate 568] [Spruce 567] [Sorbet 2658] [Squash 2661] [Tuscany 2663].**

LR: Not less than 0.83.

NRC: Not less than 0.55.

CAC: Not less than 35.

Edge/Joint Detail: SL Reveal.

Suspension Grid/Width: DX/DXL 15/16 inch (24 mm).

Panel Thickness: 3/4 inch (19 mm).

Modular Size: **[24 by 24 inches (610 by 610 mm)] [As indicated on Drawings] [As indicated in a schedule].**

Recycled Content: 69%

High Recycled Content: Classified as containing greater than 50% total recycled content. Total recycled content is based on product composition of post-consumer and pre-consumer post-industrial recycled content per FTC guidelines.

VOC Emissions: Zero-emitting performance exceeds CA Specification 01350.

Panel Features:

Firecode®, Fire rated construction, designed to meet life safety codes.

Paper back for additional performance.

Disclaimer: The USG Product Specifications contained herein are intended for use as product reference material by architects, engineers, other design professionals, contractors, building code officials, or other competent construction industry trade professionals having an interest in the selection, specification and use of products manufactured by the subsidiaries of USG Corporation. The Specifications are intended solely as technical support incident to the sale and use of USG products and not intended to be a substitute for the design review and approval of the licensed design professionals for the project. These materials may be printed and/or transferred electronically solely as needed by the user. Because electronic text files can be modified by other parties, without notice or indication of such modifications, modification of USG Product Guide Specifications and Drawings is the sole responsibility of the Design Professional.