This letter serves as certification of the recycled content of Securock® ExoAir® 430 Panel manufactured at a USG plant located at 6825 Evergreen Avenue, Jacksonville FL 32208. The panel’s baseboard is manufactured at the aforementioned plant; the panel’s membrane, which accounts for 8.4 % of dry weight of finished product is manufactured in Medina, Ohio and shipped to the Jacksonville facility for final assembly. This product is currently manufactured only at the Jacksonville plant.

USG uses more recaptured (FGD or flue gas desulfurization) gypsum than any other wallboard supplier, 2.9 million tons in 2015. However, this content changes from plant to plant and sometimes even day to day at any one plant due to availability. The recycled content provided below is based on the average production of Securock Sheathing for 2013.

**Product: Securock® ExoAir® 430 Panel  
 Pre-Consumer Recycle Content: 79.2%  
 Post-Consumer Recycle Content: 0%**

Should this be satisfactory, please specify for this project the use of Securock® ExoAir® 430 Panels. Should you have and further questions please don’t hesitate to email us at USG.4YOU-technicalsupport@usg.com or call 800 874 4968. Full product and system information can be located at www.securockexoair.com. The USG Sustainability Table can be downloaded from [www.usg.com](http://www.usg.com).

Thank you for your interest in USG products and systems.

|  |
| --- |
|  |